The red curve is the saturation line, showing the conditions under which air is at its dew point for various temperatures and humidity levels.