The red curve indicates the wet bulb temperature of the air. While related, the red curve specifically denotes saturation conditions, not just the wet bulb temperature.