The screws that have a diameter of M8 and a length of 65 mm also feature a dimension **h** of 4 mm. This specific measurement is crucial for ensuring compatibility with corresponding nuts, washers, and other fastening components in mechanical assemblies.